{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["5-delige houtspiraalborenset","5-delige houtborenset met zeska","5-delige houtborenset","5-delige hamerborenset „Pow (5)","5-delige hamerborenset „Pow (4)","5-delige hamerborenset „Pow (3)","5-delige hamerborenset „Pow (2)","5-delige hamerborenset „PowerLS","5-delige hamerborenset SDS- (2)","RESULT"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"5-delige houtspiraalborenset","index":0,"n_rows":2,"n_cols":20,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productlijn","Specificatie","Diameter mm","Diameter mm","Diameter mm","Diameter mm","Diameter mm","Schacht","bewerkbare materialen incl. detail","bewerkbare materialen incl. detail","bewerkbare materialen","bewerkbare materialen (detail)","bewerkbare materialen (detail)","Diepte mm","Breedte mm","Hoogte mm","Aantal stuks per haak van 275 mm","Aantal stuks per haak van 105 mm","Aantal stuks per haak van 165 mm"]
["2 609 255 214","Accessoires DIY","4,0; 5,0; 6,0; 8,0; 10,0 mm","4,0","5,0","6,0","8,0","10,0","cilindrisch","Holz|Hartholz/Massivholz","Holz|Weichholz","Holz","Hartholz/Massivholz","Weichholz","18","56","160","15","5","9"]

{"sheet":"5-delige houtborenset met zeska","index":1,"n_rows":2,"n_cols":22,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productlijn","Specificatie","Diameter mm","Diameter mm","Diameter mm","Diameter mm","Diameter mm","Schacht","Soort punt","Verf","bewerkbare materialen incl. detail","bewerkbare materialen incl. detail","bewerkbare materialen","bewerkbare materialen (detail)","bewerkbare materialen (detail)","Diepte mm","Breedte mm","Hoogte mm","Aantal stuks per haak van 275 mm","Aantal stuks per haak van 105 mm","Aantal stuks per haak van 165 mm"]
["2 609 255 326","Accessoires DIY","2,0; 3,0; 4,0; 5,0; 6,0 mm","2,0","3,0","4,0","5,0","6,0","Zeskant","Centreerpunt","Zwart, afschuining blank","Holz|Hartholz/Massivholz","Holz|Weichholz","Holz","Hartholz/Massivholz","Weichholz","16","57","165","17","6","10"]

{"sheet":"5-delige houtborenset","index":2,"n_rows":2,"n_cols":14,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productlijn","Titel","Productbeschrijving","Plaatsing","User benefit","","","","Inhoud","Verpakking","Afmeting (lxbxh)","Gewicht","Herkomst"]
["2 607 019 440","Promoline","5-delige Bosch houtborenset, Ø 4-10 mm.","Hoort thuis in elke gereedschapskist: Houtborenset voor precies boren in hard- en zacht hout.","Doe-het-zelven met Bosch kwaliteit: Maakt boren in hout gemakkelijk.","5 houtspiraalboren met centreerpunt voor puntzuiver aanboren.","Precieze en splintervrije boorgaten door geslepen afschuining.","Geschikt voor alle merken elektrisch gereedschap.","Veiligheidstip: Draag bij gebruik een veiligheidsbril en stofmasker.","5 houtboren, Ø 4/5/6/8/10 mm","Kunststof cassette met etiket met Euro-stansing","160 x 55 x 17","0,14 kg","China"]

{"sheet":"5-delige hamerborenset „Pow (5)","index":3,"n_rows":2,"n_cols":19,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productbenaming","Afmeting mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Schachttype"]
["F 00Y 265 101","5-delige hamerborenset „X5L” in de PowerBox","5,0 x 110/50; 6,0 x 115/50; 6,0 x 165/100; 8,0 x 165/100; 10,0 x 165/100","5,0","6,0","6,0","8,0","10,0","50","50","100","100","100","110","115","165","165","165","SDS-plus"]

{"sheet":"5-delige hamerborenset „Pow (4)","index":4,"n_rows":2,"n_cols":20,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productbenaming","Afmeting mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Schachttype","Sales Releases (voorgangers)"]
["F 00Y 266 205","5-delige hamerborenset „PowerLSplus” in PowerBox","6,0/6,0/8,0/8,0/10,0 x 165/100","6,0","6,0","8,0","8,0","10,0","100","100","100","100","100","165","165","165","165","165","SDS-plus","15"]

{"sheet":"5-delige hamerborenset „Pow (3)","index":5,"n_rows":2,"n_cols":20,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productbenaming","Afmeting mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Schachttype","Sales Releases (voorgangers)"]
["F 00Y 266 204","5-delige hamerborenset „PowerLSplus” in PowerBox","5,5/6,0/7,0/8,0/10,0 x 165/100","5,5","6,0","7,0","8,0","10,0","100","100","100","100","100","165","165","165","165","165","SDS-plus","15"]

{"sheet":"5-delige hamerborenset „Pow (2)","index":6,"n_rows":2,"n_cols":19,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productbenaming","Afmeting mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Schachttype"]
["F 00Y 266 203","5-delige hamerborenset „PowerLSplus” in PowerBox","5,0 x 115/50; 6,0 x 115/50; 6,0 x 165/100; 8,0 x 165/100; 10,0 x 165/100","5,0","6,0","6,0","8,0","10,0","50","50","100","100","100","115","115","165","165","165","SDS-plus"]

{"sheet":"5-delige hamerborenset „PowerLS","index":7,"n_rows":2,"n_cols":19,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productbenaming","Afmeting mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Schachttype"]
["F 00Y 124 424","5-delige hamerborenset „PowerLSplus” in kunststofcassette","5,0 x 110/50; 6,0 x 110/50; 6,0 x 160/100; 8,0 x 160/100; 10,0 x 160/100","5,0","6,0","6,0","8,0","10,0","50","50","100","100","100","110","110","160","160","160","SDS-plus"]

{"sheet":"5-delige hamerborenset SDS- (2)","index":8,"n_rows":2,"n_cols":18,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productlijn","Specificatie","Diameter mm x lengte mm","Diameter mm x lengte mm","Diameter mm x lengte mm","Diameter mm x lengte mm","Diameter mm x lengte mm","Schachttype","bewerkbare materialen incl. detail","bewerkbare materialen","bewerkbare materialen (detail)","Diepte mm","Breedte mm","Hoogte mm","Aantal stuks per haak van 105 mm","Aantal stuks per haak van 165 mm","Aantal stuks per haak van 275 mm"]
["2 609 255 542","Accessoires DIY","5,0x110; 5,5x110; 6,0x160; 7,0x160; 8,0x160 mm","5,0x110","5,5x110","6,0x160","7,0x160","8,0x160","SDS-plus","Beton|Beton","Beton","Beton","16","97","193","6","10","17"]

{"sheet":"RESULT","index":9,"n_rows":5,"n_cols":37,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["Bestelnummer","Productbenaming","Afmeting mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Set inhoud diameter mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Nuttige lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Totale lengte(s) mm","Schachttype","Sales Releases (voorgangers)","Productlijn","Specificatie","Diameter mm x lengte mm","Diameter mm x lengte mm","Diameter mm x lengte mm","Diameter mm x lengte mm","Diameter mm x lengte mm","Schachttype","bewerkbare materialen incl. detail","bewerkbare materialen","bewerkbare materialen (detail)","Diepte mm","Breedte mm","Hoogte mm","Aantal stuks per haak van 105 mm","Aantal stuks per haak van 165 mm","Aantal stuks per haak van 275 mm"]
["F 00Y 266 204","5-delige hamerborenset „PowerLSplus” in PowerBox","5,5/6,0/7,0/8,0/10,0 x 165/100","5,5","6,0","7,0","8,0","10,0","100","100","100","100","100","165","165","165","165","165","SDS-plus","15"]
["F 00Y 266 203","5-delige hamerborenset „PowerLSplus” in PowerBox","5,0 x 115/50; 6,0 x 115/50; 6,0 x 165/100; 8,0 x 165/100; 10,0 x 165/100","5,0","6,0","6,0","8,0","10,0","50","50","100","100","100","115","115","165","165","165","SDS-plus"]
["F 00Y 124 424","5-delige hamerborenset „PowerLSplus” in kunststofcassette","5,0 x 110/50; 6,0 x 110/50; 6,0 x 160/100; 8,0 x 160/100; 10,0 x 160/100","5,0","6,0","6,0","8,0","10,0","50","50","100","100","100","110","110","160","160","160","SDS-plus"]
["2 609 255 542",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Accessoires DIY","5,0x110; 5,5x110; 6,0x160; 7,0x160; 8,0x160 mm","5,0x110","5,5x110","6,0x160","7,0x160","8,0x160","SDS-plus","Beton|Beton","Beton","Beton","16","97","193","6","10","17"]